**K32     PANEL CUBICLES**

**120      PANEL CUBICLES – UNFRAMED**

**Manufacturer:** Formwise Washrooms Ltd, Unit 3 Wendel Point, Ryle Drive, Park Farm

Industrial Estate, Wellingborough, Northants,

NN8 6QJ. T: 01933 405961 F: 01933 405971

Email: sales@formwise-washrooms.co.uk

Web: [www.formwise-washrooms.co.uk](http://www.formise-washrooms.co.uk)

**Product reference:** ‘**ethos hpl’** toilet cubicles

**Pilasters:** Proprietary slimline pilaster profiles formed using Optisheen stainless steel. Vertical edges are fully radiused for safety with complementary stainless steel headrail fixed above pilaster profiles.

**Finish:** Satin Polished.

**Colour:** Self coloured.

**Doors:** 18mm moisture resistant chipboard faced both sides with high pressure laminate (HPL).

**Core material:** Moisture resistant chipboard (to V313).

**Finish:** Velour.

**Colour:** Colour to be confirmed from Formwise Washrooms HPL selection.

**Edge treatment:** Edges are lipped square.

**Panels:** 18mm moisture resistant chipboard faced both sides with high pressure laminate (HPL).

**Core material:** Moisture resistant chipboard (to V313).

**Finish:** Velour.

**Colour:** Colour to be confirmed from Formwise Washrooms HPL selection.

**Edge treatment:** Edges are lipped square.

**Legs:** Cylindrical stainless steel pedestal leg located on the partition 200mm back from face of adjoining pilaster. Adjustable to accommodate varying floor levels.

**Ironmongery/ Accessories:** Sprung loaded pivot hinges & dampener / Buffered coat hook / DDA compliant lever operated indicator bolt with circular face plate and emergency release facility.

**Finish/ Colour:** Stainless steel or stainless steel effect.

**Dimensions:** 2010mm overall height including 160mm floor clearance.

**Other requirements:** Complete with outward opening doors to ambulant and enlarged cubicles where requested. Cubicles with inward opening doors can be set out to maintain 450mm diameter manoeuvring space within the cubicle.